KENDALL  BREEZE  CDD

PENSACOLA

FORT WALTON BEACH

CHIPLEY

TALLAHASSEE	JACKSONVILLE
LAKE

PROPOSED ROADWAY

PANAMA CITY

CITY GAINESVILLE

ST AUGUSTINE

INDEX OF DRAINAGE REPAIR PLAN

IMPROVEMENTS

OCALA	DAYTONA BEACH DELAND

SHEET NO.
1

SHEET DESCRIPTION COVER SHEET

CITY OF MIAMI

NEW PORT RICHEY

ORLANDO BEACH LINE

MELBOURNE - COCOA

2	TABULATION OF QUANTITIES	TAMPA	LAKELAND

3-6
7-10

ROADWAY PLANS S&PM PLANS

MIAMI-DADE COUNTY, FLORIDA 33186

LOCATION OF PROJECT

ST PETERSBURG

SARASOTA - BRADENTON

BARTOW

FT PIERCE

FT MYERS

WEST PALM BEACH

SW 137TH AVE

FT LAUDERDALE MIAMI

PROJECT  LOCATION

0	1 MILE	2 MILES

SW 127TH AVE

SW 122ND AVE

SW 117TH AVE

SCALE 1"= 1 MILE

KEY WEST

Alvarez Engineers, Inc.
FLORIDA CERTIFICATE OF AUTHORIZATION No. 7538
8935 NW 35 Lane, Suite 101
Doral, Florida 33172
Tel. (305) 640-1345 Fax (305) 640-1346

GOVERNING DESIGN STANDARDS:
THESE PLANS HAVE BEEN PREPARED IN ACCORDANCE WITH AND ARE GOVERNED BY THE MIAMI-DADE COUNTY PUBLIC WORKS DEPARTMENT STANDARDS AND SPECIFICATIONS PARTS 1, 2 AND 3. THE MANUAL OF UNIFORM MINIMUM STANDARDS FOR DESIGN,
CONSTRUCTION AND MAINTENANCE FOR STREETS AND HIGHWAYS. THE FLORIDA DEPARTMENT OF TRANSPORTATION CURRENT ROADWAY AND TRAFFIC DESIGN STANDARDS, AND THE FLORIDA DEPARTMENT OF TRANSPORTATION STANDARD SPECIFICATIONS,
AS AMENDED BY CONTRACT DOCUMENTS.

LOCATION PLAN MIAMI-DADE COUNTY
T56/R40/S01&02

FEBRUARY 2025

SHEET NO.

1

Katherine Ramirez

2/13/2025

2:28:22 PM

P:\020601 - Kendall Breeze CDD (Yearly Report)\Roadway Improvements\CADD\KEYSUW01.dwg

PAY ITEM NO.	
DESCRIPTION	
UNIT		GRANO TOTAL	
					
			PLAN	FINAL	PLAN	FINAL	
0101-1	MOBILIZATION	LS					
0102-1	MAINTENANCE OF TRAFFIC	LS					
0104- 18	INLET PROTECTION SYSTEM	EA	9		9		
0110-1 -1	CLEARING & GRUBBING	AC	0.045		0.045		
0110-4-10	REMOVAL OF EXISTING CONCRETE	SY	37.8		37.8		
0120-1	REGULAR EXCAVATION	CY	33.5		33.5		
0125-3	SELECT BEDDING MATERIAL (SAND)	CY	7.3		7.3		
0285-706	OPTIONAL BASE, BASE GROUP 06 (BASEROCK)	SY	54.6		54.6		
0520-1-10	CONCRETE CURB, TYPE F	LF	75		75		
0520-2-2	CONCRETE CURB, TYPE B	LF	258		258		
0520-2-4	CONCRETE CURB, TYPED	LF	212		212		
0522-2	CONCRETE SIDEWALK AND DRIVEWAYS, 6" THICK	SY	8.7		8.7		
0526-1-2	PAVERS, ARCHITECTURAL, SIDEWALK	SY	273.0		273		
0527-2	DETECTABLE WARNINGS	SF	10.7		10.7		
0570-1-3	PERFORMANCE TURF, SOD AND SOIL- SHOULDER TREATMENT INDEX 570-010	SY	125.4		125.4		
0700- 1 - 111	SINGLE COLUMN GROUND SIGN ASSEMBLY, F&I GROUND MOUNT, LESS THAN 12 SF	EA	21		21		
0700-1-600	SINGLE COLUMN GROUND SIGN ASSEMBLY, REMOVE	EA	2		2		
0700-3-101	SIGN PANEL, FURNISH & INSTALL GROUND MOUNT, UP TO 12 SF	EA	8		8		
0700-3-501	SIGN PANEL, RELOCATE, UP TO 12 SF	EA					
0706-1-3	RAISED PAVEMENT MARKER, TYPE B	EA	288		288		
0711-11-125	THERMOPLASTIC, STANDARD, WHITE, SOLID, 24" FOR STOP LINE AND CROSSWALK	LF	81		81		
0711-11-224	THERMOPLASTIC, STANDARD, YELLOW, SOLID, 18" FOR DIAGONAL OR CHEVRON	LF	10		10		
0711-16-201	THERMOPLASTIC, STANDARD-OTHER SURFACES, YELLOW, SOLID, 6"	GM	0. 142		0. 142		

TABULATION OF	QUANTITIES	
REVISIONS	ALVAREZ ENGINEERS, INC.	
KENDALL BREEZE COO ROADWAY IMPROVEMENTS	
TABULATlION OF QUANTlITlIES	SHEET
NO.	
DATE	DESCRIPTION	DATE	DESCRIPTION					
				FLORIDA CERTIFICATE OF AUTHORIZATION No. 7538
8935 N.W.35 Lane, Suite 101
Tel.(305) Miami Florida 33172 640-1346
640-1345 Fax (305)				
							
2	

P:\FOOT\Misc Tasks\roadway\CESSROOJ .dgn : PAY ITEMSHEETS Katherine.Ramirez	2/18/2025	11 :23:38 AM

u
"l:
I.!..
'St­
a
a

"'

r,i
I

-

V)
'-.'.)
co
lLJ
..J
::::,
a::
a::
lLJ
a
:<:::,
a
lLJ
..J
<a:
lLJ
V)
a
<
<a:
a
lLJ
<
'-.'.)
vi
>­
..J
..J
<a:
;I-:;
a
lLJ
�
I.!..
�
a<
a::
I­
L,
lLJ
..J
lLJ
:lLrJ:
I-
�
1-
LIJ
:lLrJ:
V)
V)
:i:
I-
L!..
a
a a:: a
L,
lLJ
a::
..J

u

<a:
c:;:
I.!..
a
:lLrJ:
I-

u
sl'

7001111	

LL.
..,i
c:,
c:,

-

"'

r,i
I

-

Lr)
<.:)
\Q
iJJ
..J
:c:::c0
c:c
iJJ
a
<
:::0
a
iJJ
..J
"<
iJJ
l/)
a
<
"<
a
iJJ
<
<.:)
vi
>-­
..J
..J
"<
;f-:-;-
a
iJJ
�
LL.
�
<c:,
c:c
uf--­
iJJ
..J

iJJ

iJJ
:r:
f---
�

lLJ	
\.'.)	
lr)	
Q_	
fY')
("\J	
.......	
s	
lr)	

f--­
lJJ
:iJrJ:
l/)
l/)
l:
f---
LL.
c:,
a
c:c
c:,
u
icJ:cJ

..J

::::
u
w::
LL.
c:,
:iJrJ:
f---

lLJ
\.'.)
lr)
Q_
700	3101
EXIST. SIGNS	fY')
(TO REMAIN)	("\J
.......
s	N
lr)
EXIST. SIGN
(TO REMAIN}	0	5	20
\
\ \	-	Feet
\
\
EXIST. SIGN	\
(TO REMAIN)

0 ]]JI	a...
7003101	C)
1-
(.f)

{ 	_
SW 122	ST	/24" WHITE (TYP.)

�
(
"-

SW 122	ST

en
--I
700 1111	C)
--u	EXIST. SIGNS
(TO REMAIN)
700 1111	\	I	700	1111	700	3101
\	I
I	,..------ '\	I
I	I
I	I
EXIST. SIGN	I	I
(TO REMAIN)
I	I	EXIST. SIGNS (TO REMAIN)
I	I
I	I
700  3101	I	I
I	I
I	I	
REVISIONS	ALVAREZ	NGINEERS, INC.	
KENDALL BREEZE COO ROADWAY IMPROVEMENTS	
S&PM PLANS	SHEET NO.	
DATE	DESCRIPTION	DATE	DESCRIPTION					
				
FLORIDA CERTIFICATE OF AUTHORIZATION No. 7538
8935 N.W. 35 Lane, Suite IOI Miami Florida 33I 72
Tel. (305) 640-1345  Fax (305) 640-1346				

8	

P:\FDQT\Misc Tasks\roadway\PLANRO_KB _O1.d
Katherin

123 PASS - SPM [SHEET}
9:3

	

 	

ALVAREZ ENGINEERS, INC

2/18/2025

ALVAREZ ENGINEERS, INC	2/18/2025
KENDALL BREEZE CDD	
Estimate of Construction Costs
Proposed Radway Improvements	

ITEM NO.	FDOT PAY ITEM NO.	
DESCRIPTION OF WORK	
UNIT	
QUANTITY	UNIT PRICE ($/UNIT)	
COST ($)	
1	0104-18	INLET PROTECTION SYSTEM	EA	9	$	118.73	$	1,068.57	
2	0110-1-1	CLEARING & GRUBBING	AC	0.045	$ 228,836.47	$  10,297.64	
3	0110-4-10	REMOVAL OF EXISTING CONCRETE	SY	37.8	$	34.64	$	1,309.39	
4	0120-1	REGULAR EXCAVATION	CY	33.5	$	16.08	$	537.91	
5	0125-3	SELECT BEDDING MATERIAL (SAND)	CY	7.3	$	1,000.00	$	7,279.88	
6	0285-706	OPTIONAL BASE, BASE GROUP 06 (BASEROCK)	SY	54.6	$	17.00	$	928.18	
7	0520-1-10	CONCRETE CURB, TYPE F	LF	75	$	42.46	$	3,184.50	
8	0520-2-2	CONCRETE CURB, TYPE B	LF	258	$	112.22	$  28,952.76	
9	0520-2-4	CONCRETE CURB, TYPE D	LF	212	$	38.53	$	8,168.36	
10	0522-2	CONCRETE SIDEWALK AND DRIVEWAYS, 6" THICK	SY	8.7	$	86.39	$	751.59	
11	0526-1-2	PAVERS, ARCHITECTURAL, SIDEWALK	SY	273	$	67.59	$  18,452.07	
12	0527-2	DETECTABLE WARNINGS	SF	10.7	$	41.28	$	441.70	
13	0570-1-3	PERFORMANCE TURF, SOD AND SOIL- SHOULDER TREATMENT INDEX 570-010	SY	125.4	$	8.05	$	1,009.47	
14	0700-1-111	SINGLE COLUMN GROUND SIGN ASSEMBLY, F&I GROUND MOUNT, LESS THAN 12 SF	EA	21	$	444.48	$	9,334.08	
15	0700-1-600	SINGLE COLUMN GROUND SIGN ASSEMBLY, REMOVE	EA	2	$	39.40	$	78.80	
16	0700-3-101	SIGN PANEL, FURNISH & INSTALL GROUND MOUNT, UP TO 12 SF	EA	8	$	280.62	$	2,244.96	
17	0700-3-501	SIGN PANEL, RELOCATE, UP TO 12 SF	EA	1	$	142.39	$	142.39	
18	0706-1-3	RAISED PAVEMENT MARKER, TYPE B	EA	288	$	4.52	$	1,301.76	
19	0711-11-125	THERMOPLASTIC, STANDARD, WHITE, SOLID, 24" FOR STOP LINE AND CROSSWALK	LF	81	$	5.10	$	413.10	
20	0711-11-224	THERMOPLASTIC, STANDARD, YELLOW, SOLID, 18" FOR DIAGONAL OR CHEVRON	LF	10	$	3.90	$	39.00	
21	0711-16-201	THERMOPLASTIC, STANDARD-OTHER SURFACES, YELLOW, SOLID, 6"	GM	0.142	$	5,972.61	$	848.11	
							
PARKING WIDENING SUBTOTAL	$  96,784.22	
22	-	CONTINGENCY (20%)	LS	1	$  19,356.84	$  19,356.84	
23	101-1	MOBILIZATION (20%)	LS	1	$  19,356.84	$  19,356.84	
24	102-1	MAINTENANCE OF TRAFFIC (5%)	LS	1	$	9,678.42	$	9,678.42	
GENERAL SUBTOTAL	$ 145,176.32	
GRAND TOTAL	$ 146,000.00